**Porous Silicon: A Buffer Layer for PbS Heteroepitaxy**

**V. Yakovtseva 1**

**N. Vorozov 2**

**L. Dolgyi 3**

**V. Levchenko 4**

**L. Postnova 5**

**M. Balucani 6**

**V. Bondarenko 7**

**G. Lamedica 8**

**V. Ferrara 9**

**A. Ferrari 10**

1, 7 Belarusian State University of Informatics and Radio Electronics

**Abstract.** In the present work, we report on the heteroepitaxial growth of PbS on porous silicon (PS). Epitaxial PbS films were grown by MBE on the surface of PS formed on the n+-type silicon (111) substrate. The films were comparable with films grown on BaF2 substrates. Beneficial influence of a PS buffer layer on the structure and properties of PbS epitaxial films was supported by implementation of sensitive Schottky-barrier photodiodes fabricated in these films.

**Keywords:** porous silicon.

**DOI:** 10.1002/1521-396X(200011)182:1<195::AID-PSSA195>3.0.CO;2-G

[http://onlinelibrary.wiley.com/doi/10.1002/1521-396X(200011)182:1<195::AID-PSSA195>3.0.CO;2-G/abstract](http://onlinelibrary.wiley.com/doi/10.1002/1521-396X%28200011%29182%3A1%3C195%3A%3AAID-PSSA195%3E3.0.CO%3B2-G/abstract)