Sol-gel fabrication of zinc oxide nanostructured coatings on a fiberglass tissue

T. A. Filippova1,

 V. E. Borisenko2,

V. V. Uglov3,

 S. V. Zlotski4

2017 г.

1 Belarusian State University, Nezavisimosti Ave. 4, 220030 Minsk, Belarus

2 Tomsk Polytechnic University, Lenina Ave. 2a, 634028 Tomsk, Russia

3 Belarusian State University of Informatics and Radioelectronics P. Browka 6, 220013 Minsk, Belarus

**Ключевые слова:** nanostructures, sol-gel technology, zinc oxide, fiberglass tissue

**Abstract/Аннотация:** Nanostructured zinc oxide coatings were for the first time fabricated by sol-gel technique on a fiberglass tissue. The coatings have demonstrated high catalytic activity in UV light assisted decomposition of Rhodamine B.

**Источник публикации:** Sol-gel fabrication of zinc oxide nanostructured coatings on a fiberglass tissue / T. A. Filippova [etc] // Physics, Chemistry and Application of Nanostructures. – edited by V. E. Borisenko, S. V. Gaponenko, V. S. Gurin, C. H. Kam (World Scientific, Singapore, 2017). – pp. 365-368.

**Read More:**

http://www.worldscientific.com/worldscibooks/10.1142/10560

<http://www.worldscientific.com/doi/pdf/10.1142/9789813224537_0084>